**Apparel Check List (General Use)**

**(clothing, wearables, sashes, hats, scarves, mittons)**

**Garment Requirements**

Lead Content in Paint and Similar Surface Coatings (16 CFR 1303)

Total Cadmium in clothing (Detachable ornaments which are similar to an anklet, arm cuff, bracelet, charm, brooch, chain, crown, cuff link, watch: <300 ppm)

Flame Retardants: PentaBDE, OctaBDE, DecaBDE, TCEP. No detection.

Fiber Content/Analysis AATCC 20/20A

*Testing not required if vendor provides data.*

Flammability of wearing apparel. 16 CFR 1610

Flammability of vinyl material. 16 CFR 1611

*Testing not required if no vinyl present in garment.*

Flammability of Solids. 16 CFR 1500.44

*Testing not required unless accessories present.*

Drawstrings (No drawstrings in the hood and neck area ; drawstrings at waist and bottom may not extend more than 3” past channel when garmet is expanded to fullest width; no toggles, knots or other atttachments at free ends; bartacked if drawstring is one continuous string (applies to products intended for individuals up to 16 years of age, including age 16)

Care Labeling. 16 CFR 423

*Testing not required and a visual inspection is ok provided the vendor provides the information.*

Textile Fiber Products Identification/RN#.16 CFR 303/300

*Testing not required; visual inspection ok.*

Country of Origin Marking. 19 CFR 134.11

*Testing not required; visual inspection ok.*

General Certificate of Conformity (“GCC”)

Recent Test Report

**California Prop 65**

Lead in Substrates and Surface Coatings <90 ppm

*May use CPSIA lead testing data. Additional testing typically not required.*

Phthalates (DBP, BBP, DEHP, DINP, DIDP, DnHP)

*Testing may not be necessary if no plastic components. Consult with Anseco on a case by case basis.*

Total Cadmium in Surface Coatings and Substrates

Bisphenol A (BPA) (<100PPT)

***A warning label on the product, packaging and marketing materials will be required for products going into California if phthalates/Cadmium/BPH is in excess of the safe harbor limits. If lead is in excess of the 90/100 ppm, the product may not be sold anywhere in the United States as the product would be deemed a banned hazardous substance.***

**Packaging Requirements**

TPCH/Coneg/Toxic Elements in Packaging Material (sum of cadmium, hexavalent chromium, lead and mercury in packaging and packaging components shall be < 100ppm by weight)

Plastic Bag Warning. **“Warning: To avoid danger of suffocation, keep this plastic bag away from babies and children. Do not use this bag in cribs, beds, carriages or playpens. This bag is not a toy.”**

*Testing not required; visual inspection is ok.*

Prop 65 Warning Label if phthalates, cadmium and/or BPA in excess of the safe harbor limits is present.

**Marketing Material Requirements**

Prop 65 Warning Labels (including on websites, catalogs)

Version Control

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Version** | **Description** | **Document #** | **Effective Date** | **Created by:** |
| 1 | Apparel Check List (General Use) | 902121\_1 | 07/20/2016 | Emily Rudie |
| 2 | Apparel Check List (General Use)   * Clothing, wearables, sashes, hats, scarves, mittons, added to description | 902121\_2 | 07/21/2016 | Emily Rudie |