**Jewelry\* Check List (Children’s)**

**(wristbands, dog tags)**

**Product Requirements**

[ ]  Lead in Paints and Surface Coatings. 16 CFR 1303, CPSIA Section 101, ASTM F2923-5 (<90ppm)

 [ ]  Test conducted by Accredited Third Party Lab.

[ ]  Testing was conducted within the past 12 months.

[ ]  If lead measures between 40ppm – 90 ppm, IL warning required.

*Testing not required if the article contains no surface coatings/paints.*

[ ]  Total Lead in Substrates. CPSIA Section 101, ASTM F2923.5 (<100ppm).

 [ ]  Test conducted by Accredited Third Party Lab.

[ ]  Testing was conducted within the past 12 months.

[ ]  If lead measures between 40ppm – 90 ppm, IL warning required.

[ ]  Total Lead Content – ASTM F2923-14.

*Testing may not be required if Anseco confirms CPSIA lead test can be used.*

[ ]  Soluble Heavy Metals in Paint and Surface Coatings. ASTM F2923-14.

[ ]  Total Cadmium in Substrates. ASTM F2923-14.

[ ]  Nickel Release. ASTM F2923-14.

[ ]  Jewelry Mechanical Hazards. ASTM F2923.14.

[ ]  Jewelry Labeling. ASTM F2923-14.

[ ]  Flammability of Solids. 16 CFR 1500.44

 *Testing not required unless accessories present.*

[ ]  Formaldehyde in Children’s Products. Minnesota 325F, Sec. 176-178. No detectable levels.

 *May not be relevant. Consult with Anseco*

[ ]  Sharp Points. 16 CFR 1500.48

*Testing may not be required if Anseco advises that the Mechanical tests for ASTM F2923-14 may be relied upon*

[ ]  Sharp Points (Metal or Glass). 16 CFR 1500.49

*Testing may not be required if Anseco advises that the Mechanical tests for ASTM F2923-14 may be relied upon*.

[ ]  Tracking Label. CPSIA 103;

 *Testing not required. Visual inspection is ok.*

* Permanently affixed to product
* Name of Manufacturer
* Location of Manufacture
* Date of Manufacture
* Unique Tracking Number

[ ]  Country of Origin Marking. 19 CFR 134.11

 *Testing not required; visual inspection ok.*

[ ]  Children’s Product Certificate

[ ]  Recent Test Report (less than 12 months old)

[ ]  Washington Children’s Safe Product Act Total Cadmium in Surface Coatings and Substrates.

[ ]  Washington Children’s Safe Product Act Phthalate Content (DEHP, DBP, BBP, DINP, DIDP, DnOP)

[ ]  Warning Labels. Small parts, magnets, etc.

**California Prop 65**

[ ]  Lead in Substrates and Surface Coatings <90 ppm

*May use CPSIA lead testing data. Additional testing typically not required.*

[ ]  Phthalates (DBP, BBP, DEHP, DINP, DIDP, DnHP)

*Testing may not be necessary if no plastic components. Consult with Anseco on a case by case basis.*

[ ]  Total Cadmium in Surface Coatings and Substrates

[ ]  Bisphenol A (BPA) (<100PPT)

***A warning label on the product, packaging and marketing materials will be required for products going into California if phthalates/Cadmium/BPH is in excess of the safe harbor limits. If lead is in excess of the 90/100 ppm, the product may not be sold anywhere in the United States as the product would be deemed a banned hazardous substance.***

**Washington Children’s Safe Products Act 70.240**

*(Applicable to any of the following: toys, children’s cosmetics, children’s jewelry, product used to help a child suck, teeth, sleep, relax, feed, worn as clothing by children, or car seats. Applies to children 12 years of age or younger).*

[ ]  Lead <90ppm in product or product component

[ ]  Cadmium <40ppm in product or product component

[ ]  Phthalates, individually or combined, <1000 ppm in product or product component.

[ ]  Registration if the Children’s Product contains any of the High Priority Chemicals

**Packaging Requirements**

[ ]  TPCH/Coneg/Toxic Elements in Packaging Material (sum of cadmium, hexavalent chromium, lead and mercury in packaging and packaging components shall be < 100ppm by weight)

[ ]  Plastic Bag Warning. **“Warning: To avoid danger of suffocation, keep this plastic bag away from babies and children. Do not use this bag in cribs, beds, carriages or playpens. This bag is not a toy.”**

*Testing not required; visual inspection is ok.*

[ ]  Warning Labels. Small parts, magnets, etc.

 *Testing not required, visual inspection ok.*

[ ]  Prop 65 Warning Label if phthalates, cadmium and/or BPA in excess of the safe harbor limits is present.

 *Testing not required; visual inspection is ok.*

[ ]  Tracking Label

 *Testing not required; visual inspection is ok.*

[ ]  Jewelry Label Claims. 16 CFR 23 (i.e. silver vs. silver plated; gold vs. gold colored.)

[ ]  Age Labeling of Children’s Jewelry. ASTM F2923-4. “Jewelry is not recommended for children under 3 except under close parental supervision.”

[ ]  Country of Origin

**Marketing Material Requirements**

[ ]  Warning Labels. If applicable, must be on all marketing materials (website, catalogs, etc.)

[ ]  Prop 65 Warning Labels (including on websites, catalogs)

[ ]  Jewelry Label Claims. 16 CFR 23 (i.e. silver vs. silver plated; gold vs. gold colored.)

[ ]  Age Labeling of Children’s Jewelry. ASTM F2923-4. “Jewelry is not recommended for children under 3 except under close parental supervision.”

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Version** | **Description** | **Document #** | **Effective Date** | **Created by:** |
| 1 | Children’s Jewelry – Checklist | 889839\_1 | 4/29/2016 | Emily Rudie |
| 2 | Jewelry Check List (Children’s)* Country of Origin added
 | 889839\_2 | 07/20/2016 | Emily Rudie |
| 3 | Jewelry Check List (Children’s)* Wristbands added
* Dog Tags added
 | 889839\_3 | 07/21/2016 | Emily Rudie |